TV	Rainford TV5588SC
Chas	M11
PCB	MITPC20205-M11D
µCom	M37221M4-322SP
Vid	M52771ASP
SAW	K2966M
Vert	LA7840
FBT	S20007-H01A (S14010-H01A)
HOT	ST1803DHI
SMPS	STR-S6707, TLP721F, TL431
Audio	TDA2616
Tuner	WV05I-212A
RC	RP-10

Serv	Press “DISPLAY” and “VSM” key simultaneously from the RC
	Press “DISPLAY” key to memorize the service setting and come
	out of the service mode