TV	Start 2166P
Chas	
PCB
********************
µÑom	LC863328B 52E5
Memory	24C08
Dump	Start_2166P.bin
********************
SMPS	2SD1710C
FBT	BSC 25-0108W www.c-fbt.com
HOT	2SD1651C
Vert	LA7840
Vid	LA76810A/LA7642N
SAW	LS F38,9C1
Tuner	ET-5C1E-EV200T
Voice	AN5265

Service	Press hide keys on RC
	or 
	Press Recall key on RC, Than
	press Vol- key on TV, lock it,
	and come time press Recall key on RC